**Depth Camera D435**

|  |  |
| --- | --- |
| **Depth** | **Depth Technology:**  **Active IR Stereo  Depth Field of View (FOV): 87°±3° x 58°±1° x 95°±3°**  **Minimum Depth Distance (Min-Z): 0.105 m  Depth Output Resolution & Frame Rate: Up to 1280 x 720 active stereo depth resolution. Up to 90 fps.** |
| **RGB** | **RGB Sensor FOV (H x V x D):** 69.4° x 42.5° x 77° (+/- 3°)  **RGB Sensor Resolution & Frame Rate:** 1920 x 1080. 30 fps |